#!/bin/sh
. /etc/functions.sh
. /etc/network.overrides
[ "$FAILSAFE" != "true" -a -e /etc/config/network ] && . /etc/config/network

WAN=$(nvram get wan_ifname)
LAN=$(nvram get lan_ifname)

iptables -F input_rule
iptables -F output_rule
iptables -F forwarding_rule
iptables -t nat -F prerouting_rule
iptables -t nat -F postrouting_rule

### BIG FAT DISCLAIMER
### The "-i $WAN" literally means packets that came in over the $WAN interface;
### this WILL NOT MATCH packets sent from the LAN to the WAN address.

### Allow SSH on the WAN interface
# iptables -t nat -A prerouting_rule -i $WAN -p tcp --dport 22 -j ACCEPT 
# iptables        -A input_rule      -i $WAN -p tcp --dport 22 -j ACCEPT

### Port forwarding
# iptables -t nat -A prerouting_rule -i $WAN -p tcp --dport 22 -j DNAT --to 192.168.1.2
# iptables        -A forwarding_rule -i $WAN -p tcp --dport 22 -d 192.168.1.2 -j ACCEPT

### DMZ (should be placed after port forwarding / accept rules)
# iptables -t nat -A prerouting_rule -i $WAN -j DNAT --to 192.168.1.2
# iptables        -A forwarding_rule -i $WAN -d 192.168.1.2 -j ACCEPT
