--- a/arch/mips/lantiq/xway/devices.c
+++ b/arch/mips/lantiq/xway/devices.c
@@ -154,6 +154,26 @@
 	lantiq_emulate_madwifi_eep = 1;
 }
 
+/* gpio buttons */
+static struct gpio_buttons_platform_data ltq_gpio_buttons_platform_data;
+
+static struct platform_device ltq_gpio_buttons_platform_device =
+{
+	.name = "gpio-buttons",
+	.id = 0,
+	.dev = {
+		.platform_data = (void *) &ltq_gpio_buttons_platform_data,
+	},
+};
+
+void __init
+ltq_register_gpio_buttons(struct gpio_button *buttons, int cnt)
+{
+	ltq_gpio_buttons_platform_data.buttons = buttons;
+	ltq_gpio_buttons_platform_data.nbuttons = cnt;
+	platform_device_register(&ltq_gpio_buttons_platform_device);
+}
+
 static struct resource ltq_spi_resources[] = {
 	{
 		.start  = LTQ_SSC_BASE_ADDR,
--- a/arch/mips/lantiq/xway/devices.h
+++ b/arch/mips/lantiq/xway/devices.h
@@ -11,6 +11,7 @@
 
 #include "../devices.h"
 #include <linux/phy.h>
+#include <linux/gpio_buttons.h>
 
 extern void ltq_register_gpio(void);
 extern void ltq_register_gpio_stp(void);
@@ -18,5 +19,6 @@
 extern void ltq_register_etop(struct ltq_eth_data *eth);
 extern void ltq_register_gpio_ebu(unsigned int value);
 extern void ltq_register_madwifi_eep(void);
+extern void ltq_register_gpio_buttons(struct gpio_button *buttons, int cnt);
 
 #endif
