From e6a1210bef8b48a946f1afb6d951f4b2448219ac Mon Sep 17 00:00:00 2001
From: Rene Bolldorf <xsecute@googlemail.com>
Date: Fri, 18 Nov 2011 00:17:42 +0000
Subject: [PATCH 18/27] Initial support for the Ubiquiti Networks XM board (rev 1.0).

Signed-off-by: Rene Bolldorf <xsecute@googlemail.com>
Cc: linux-mips@linux-mips.org
Cc: linux-kernel@vger.kernel.org
Patchwork: https://patchwork.linux-mips.org/patch/3020/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ath79/Kconfig        |   11 ++++
 arch/mips/ath79/Makefile       |    1 +
 arch/mips/ath79/mach-ubnt-xm.c |  119 ++++++++++++++++++++++++++++++++++++++++
 arch/mips/ath79/machtypes.h    |    1 +
 4 files changed, 132 insertions(+), 0 deletions(-)
 create mode 100644 arch/mips/ath79/mach-ubnt-xm.c

--- a/arch/mips/ath79/Kconfig
+++ b/arch/mips/ath79/Kconfig
@@ -36,6 +36,16 @@ config ATH79_MACH_PB44
 	  Say 'Y' here if you want your kernel to support the
 	  Atheros PB44 reference board.
 
+config ATH79_MACH_UBNT_XM
+	bool "Ubiquiti Networks XM (rev 1.0) board"
+	select SOC_AR724X
+	select ATH79_DEV_GPIO_BUTTONS
+	select ATH79_DEV_LEDS_GPIO
+	select ATH79_DEV_SPI
+	help
+	  Say 'Y' here if you want your kernel to support the
+	  Ubiquiti Networks XM (rev 1.0) board.
+
 endmenu
 
 config SOC_AR71XX
@@ -46,6 +56,7 @@ config SOC_AR71XX
 config SOC_AR724X
 	select USB_ARCH_HAS_EHCI
 	select USB_ARCH_HAS_OHCI
+	select HW_HAS_PCI
 	def_bool n
 
 config SOC_AR913X
--- a/arch/mips/ath79/Makefile
+++ b/arch/mips/ath79/Makefile
@@ -28,3 +28,4 @@ obj-$(CONFIG_ATH79_DEV_USB)		+= dev-usb.
 obj-$(CONFIG_ATH79_MACH_AP121)		+= mach-ap121.o
 obj-$(CONFIG_ATH79_MACH_AP81)		+= mach-ap81.o
 obj-$(CONFIG_ATH79_MACH_PB44)		+= mach-pb44.o
+obj-$(CONFIG_ATH79_MACH_UBNT_XM)	+= mach-ubnt-xm.o
--- /dev/null
+++ b/arch/mips/ath79/mach-ubnt-xm.c
@@ -0,0 +1,119 @@
+/*
+ *  Ubiquiti Networks XM (rev 1.0) board support
+ *
+ *  Copyright (C) 2011 René Bolldorf <xsecute@googlemail.com>
+ *
+ *  Derived from: mach-pb44.c
+ *
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ */
+
+#include <linux/init.h>
+#include <linux/pci.h>
+
+#ifdef CONFIG_PCI
+#include <linux/ath9k_platform.h>
+#include <asm/mach-ath79/pci-ath724x.h>
+#endif /* CONFIG_PCI */
+
+#include "machtypes.h"
+#include "dev-gpio-buttons.h"
+#include "dev-leds-gpio.h"
+#include "dev-spi.h"
+
+#define UBNT_XM_GPIO_LED_L1		0
+#define UBNT_XM_GPIO_LED_L2		1
+#define UBNT_XM_GPIO_LED_L3		11
+#define UBNT_XM_GPIO_LED_L4		7
+
+#define UBNT_XM_GPIO_BTN_RESET		12
+
+#define UBNT_XM_KEYS_POLL_INTERVAL	20
+#define UBNT_XM_KEYS_DEBOUNCE_INTERVAL	(3 * UBNT_XM_KEYS_POLL_INTERVAL)
+
+#define UBNT_XM_PCI_IRQ			48
+#define UBNT_XM_EEPROM_ADDR		(u8 *) KSEG1ADDR(0x1fff1000)
+
+static struct gpio_led ubnt_xm_leds_gpio[] __initdata = {
+	{
+		.name		= "ubnt-xm:red:link1",
+		.gpio		= UBNT_XM_GPIO_LED_L1,
+		.active_low	= 0,
+	}, {
+		.name		= "ubnt-xm:orange:link2",
+		.gpio		= UBNT_XM_GPIO_LED_L2,
+		.active_low	= 0,
+	}, {
+		.name		= "ubnt-xm:green:link3",
+		.gpio		= UBNT_XM_GPIO_LED_L3,
+		.active_low	= 0,
+	}, {
+		.name		= "ubnt-xm:green:link4",
+		.gpio		= UBNT_XM_GPIO_LED_L4,
+		.active_low	= 0,
+	},
+};
+
+static struct gpio_keys_button ubnt_xm_gpio_keys[] __initdata = {
+	{
+		.desc			= "reset",
+		.type			= EV_KEY,
+		.code			= KEY_RESTART,
+		.debounce_interval	= UBNT_XM_KEYS_DEBOUNCE_INTERVAL,
+		.gpio			= UBNT_XM_GPIO_BTN_RESET,
+		.active_low		= 1,
+	}
+};
+
+static struct spi_board_info ubnt_xm_spi_info[] = {
+	{
+		.bus_num	= 0,
+		.chip_select	= 0,
+		.max_speed_hz	= 25000000,
+		.modalias	= "mx25l6405d",
+	}
+};
+
+static struct ath79_spi_platform_data ubnt_xm_spi_data = {
+	.bus_num		= 0,
+	.num_chipselect		= 1,
+};
+
+#ifdef CONFIG_PCI
+static struct ath9k_platform_data ubnt_xm_eeprom_data;
+
+static struct ath724x_pci_data ubnt_xm_pci_data[] = {
+	{
+		.irq	= UBNT_XM_PCI_IRQ,
+		.pdata	= &ubnt_xm_eeprom_data,
+	},
+};
+#endif /* CONFIG_PCI */
+
+static void __init ubnt_xm_init(void)
+{
+	ath79_register_leds_gpio(-1, ARRAY_SIZE(ubnt_xm_leds_gpio),
+				 ubnt_xm_leds_gpio);
+
+	ath79_register_gpio_keys_polled(-1, UBNT_XM_KEYS_POLL_INTERVAL,
+					ARRAY_SIZE(ubnt_xm_gpio_keys),
+					ubnt_xm_gpio_keys);
+
+	ath79_register_spi(&ubnt_xm_spi_data, ubnt_xm_spi_info,
+			   ARRAY_SIZE(ubnt_xm_spi_info));
+
+#ifdef CONFIG_PCI
+	memcpy(ubnt_xm_eeprom_data.eeprom_data, UBNT_XM_EEPROM_ADDR,
+	       sizeof(ubnt_xm_eeprom_data.eeprom_data));
+
+	ath724x_pci_add_data(ubnt_xm_pci_data, ARRAY_SIZE(ubnt_xm_pci_data));
+#endif /* CONFIG_PCI */
+
+}
+
+MIPS_MACHINE(ATH79_MACH_UBNT_XM,
+	     "UBNT-XM",
+	     "Ubiquiti Networks XM (rev 1.0) board",
+	     ubnt_xm_init);
--- a/arch/mips/ath79/machtypes.h
+++ b/arch/mips/ath79/machtypes.h
@@ -19,6 +19,7 @@ enum ath79_mach_type {
 	ATH79_MACH_AP121,		/* Atheros AP121 reference board */
 	ATH79_MACH_AP81,		/* Atheros AP81 reference board */
 	ATH79_MACH_PB44,		/* Atheros PB44 reference board */
+	ATH79_MACH_UBNT_XM,		/* Ubiquiti Networks XM board rev 1.0 */
 };
 
 #endif /* _ATH79_MACHTYPE_H */
