From 3cd3138f2ef77e18abc99737c6740f35d61dbbb3 Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Sun, 15 Jan 2012 23:05:05 +0100
Subject: [PATCH 26/32] bcma: make some functions __devinit

bcma_core_pci_hostmode_init() has to be in __devinit as it will call a
function in that section and so all functions calling it also have to
be in __devinit.

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 drivers/bcma/bcma_private.h          |    4 ++--
 drivers/bcma/driver_pci.c            |    6 +++---
 drivers/bcma/driver_pci_host.c       |    2 +-
 drivers/bcma/host_pci.c              |    4 ++--
 drivers/bcma/main.c                  |    2 +-
 include/linux/bcma/bcma_driver_pci.h |    2 +-
 6 files changed, 10 insertions(+), 10 deletions(-)

--- a/drivers/bcma/bcma_private.h
+++ b/drivers/bcma/bcma_private.h
@@ -13,7 +13,7 @@
 struct bcma_bus;
 
 /* main.c */
-int bcma_bus_register(struct bcma_bus *bus);
+int __devinit bcma_bus_register(struct bcma_bus *bus);
 void bcma_bus_unregister(struct bcma_bus *bus);
 int __init bcma_bus_early_register(struct bcma_bus *bus,
 				   struct bcma_device *core_cc,
@@ -60,7 +60,7 @@ extern void __exit bcma_host_pci_exit(vo
 #endif /* CONFIG_BCMA_HOST_PCI */
 
 #ifdef CONFIG_BCMA_DRIVER_PCI_HOSTMODE
-void bcma_core_pci_hostmode_init(struct bcma_drv_pci *pc);
+void __devinit bcma_core_pci_hostmode_init(struct bcma_drv_pci *pc);
 #endif /* CONFIG_BCMA_DRIVER_PCI_HOSTMODE */
 
 #endif
--- a/drivers/bcma/driver_pci.c
+++ b/drivers/bcma/driver_pci.c
@@ -174,12 +174,12 @@ static void bcma_pcicore_serdes_workarou
  * Init.
  **************************************************/
 
-static void bcma_core_pci_clientmode_init(struct bcma_drv_pci *pc)
+static void __devinit bcma_core_pci_clientmode_init(struct bcma_drv_pci *pc)
 {
 	bcma_pcicore_serdes_workaround(pc);
 }
 
-static bool bcma_core_pci_is_in_hostmode(struct bcma_drv_pci *pc)
+static bool __devinit bcma_core_pci_is_in_hostmode(struct bcma_drv_pci *pc)
 {
 	struct bcma_bus *bus = pc->core->bus;
 	u16 chipid_top;
@@ -204,7 +204,7 @@ static bool bcma_core_pci_is_in_hostmode
 	return true;
 }
 
-void bcma_core_pci_init(struct bcma_drv_pci *pc)
+void __devinit bcma_core_pci_init(struct bcma_drv_pci *pc)
 {
 	if (pc->setup_done)
 		return;
--- a/drivers/bcma/driver_pci_host.c
+++ b/drivers/bcma/driver_pci_host.c
@@ -8,7 +8,7 @@
 #include "bcma_private.h"
 #include <linux/bcma/bcma.h>
 
-void bcma_core_pci_hostmode_init(struct bcma_drv_pci *pc)
+void __devinit bcma_core_pci_hostmode_init(struct bcma_drv_pci *pc)
 {
 	pr_err("No support for PCI core in hostmode yet\n");
 }
--- a/drivers/bcma/host_pci.c
+++ b/drivers/bcma/host_pci.c
@@ -154,8 +154,8 @@ const struct bcma_host_ops bcma_host_pci
 	.awrite32	= bcma_host_pci_awrite32,
 };
 
-static int bcma_host_pci_probe(struct pci_dev *dev,
-			     const struct pci_device_id *id)
+static int __devinit bcma_host_pci_probe(struct pci_dev *dev,
+					 const struct pci_device_id *id)
 {
 	struct bcma_bus *bus;
 	int err = -ENOMEM;
--- a/drivers/bcma/main.c
+++ b/drivers/bcma/main.c
@@ -132,7 +132,7 @@ static void bcma_unregister_cores(struct
 	}
 }
 
-int bcma_bus_register(struct bcma_bus *bus)
+int __devinit bcma_bus_register(struct bcma_bus *bus)
 {
 	int err;
 	struct bcma_device *core;
--- a/include/linux/bcma/bcma_driver_pci.h
+++ b/include/linux/bcma/bcma_driver_pci.h
@@ -169,7 +169,7 @@ struct bcma_drv_pci {
 #define pcicore_read32(pc, offset)		bcma_read32((pc)->core, offset)
 #define pcicore_write32(pc, offset, val)	bcma_write32((pc)->core, offset, val)
 
-extern void bcma_core_pci_init(struct bcma_drv_pci *pc);
+extern void __devinit bcma_core_pci_init(struct bcma_drv_pci *pc);
 extern int bcma_core_pci_irq_ctl(struct bcma_drv_pci *pc,
 				 struct bcma_device *core, bool enable);
 
