--- a/arch/mips/lantiq/machtypes.h
+++ b/arch/mips/lantiq/machtypes.h
@@ -32,6 +32,9 @@
 	LANTIQ_MACH_ARV752DPW,		/* Arcor easybox a802 */
 	LANTIQ_MACH_ARV752DPW22,	/* Arcor easybox a803 */
 	LANTIQ_MACH_ARV7518PW,		/* ASTORIA */
+
+	/* Netgear */
+	LANTIQ_MACH_DGN3500B,		/* Netgear DGN3500 */
 };
 
 #endif
--- a/arch/mips/lantiq/xway/Kconfig
+++ b/arch/mips/lantiq/xway/Kconfig
@@ -10,6 +10,10 @@
 	bool "ARV45XX"
 	default y
 
+config LANTIQ_MACH_NETGEAR
+	bool "Netgear"
+	default y
+
 endmenu
 
 endif
--- a/arch/mips/lantiq/xway/Makefile
+++ b/arch/mips/lantiq/xway/Makefile
@@ -6,4 +6,5 @@
 obj-$(CONFIG_LANTIQ_MACH_EASY50712) += mach-easy50712.o
 obj-$(CONFIG_LANTIQ_MACH_EASY50601) += mach-easy50601.o
 obj-$(CONFIG_LANTIQ_MACH_ARV45XX) += mach-arv45xx.o
+obj-$(CONFIG_LANTIQ_MACH_NETGEAR) += mach-netgear.o
 obj-y += dev-dwc_otg.o
--- a/arch/mips/lantiq/xway/devices.h
+++ b/arch/mips/lantiq/xway/devices.h
@@ -12,6 +12,7 @@
 #include "../devices.h"
 #include <linux/phy.h>
 #include <linux/gpio_buttons.h>
+#include <linux/spi/spi.h>
 
 extern void ltq_register_gpio(void);
 extern void ltq_register_gpio_stp(void);
@@ -20,5 +21,7 @@
 extern void ltq_register_gpio_ebu(unsigned int value);
 extern void ltq_register_madwifi_eep(void);
 extern void ltq_register_gpio_buttons(struct gpio_button *buttons, int cnt);
+extern void ltq_register_spi(struct ltq_spi_platform_data *pdata,
+		struct spi_board_info const *info, unsigned n);
 
 #endif
--- /dev/null
+++ b/arch/mips/lantiq/xway/mach-netgear.c
@@ -0,0 +1,57 @@
+/*
+ *  This program is free software; you can redistribute it and/or modify it
+ *  under the terms of the GNU General Public License version 2 as published
+ *  by the Free Software Foundation.
+ *
+ *  Copyright (C) 2010 John Crispin <blogic@openwrt.org>
+ */
+
+#include <linux/init.h>
+#include <linux/platform_device.h>
+#include <linux/mtd/mtd.h>
+#include <linux/mtd/partitions.h>
+#include <linux/mtd/physmap.h>
+#include <linux/input.h>
+#include <linux/phy.h>
+#include <linux/spi/spi.h>
+
+#include <lantiq_soc.h>
+#include <irq.h>
+
+#include "../machtypes.h"
+#include "devices.h"
+
+static struct ltq_pci_data ltq_pci_data = {
+	.clock	= PCI_CLOCK_INT,
+	.gpio	= PCI_GNT1 | PCI_REQ1,
+	.irq	= {
+		[14] = INT_NUM_IM0_IRL0 + 22,
+	},
+};
+
+static struct ltq_eth_data ltq_eth_data = {
+	.mii_mode = PHY_INTERFACE_MODE_MII,
+};
+
+struct spi_board_info spi_info = {
+	.bus_num        = 0,
+	.chip_select    = 3,
+	.max_speed_hz   = 25000000,
+	.modalias       = "mx25l12805d",
+};
+
+struct ltq_spi_platform_data ltq_spi_data = {
+	.num_chipselect = 4,
+};
+
+static void __init dgn3500_init(void)
+{
+	ltq_register_pci(&ltq_pci_data);
+	ltq_register_etop(&ltq_eth_data);
+	ltq_register_spi(&ltq_spi_data, &spi_info, 1);
+}
+
+MIPS_MACHINE(LANTIQ_MACH_DGN3500B,
+	     "DGN3500B",
+	     "Netgear DGN3500B",
+	      dgn3500_init);
