From: Benoit Cousson <b-cousson@ti.com>
Date: Sat, 17 Dec 2011 00:09:11 +0000 (-0800)
Subject: ARM: OMAP4: hwmod: Don't wait for the idle status if modulemode is not supported
X-Git-Url: http://git.kernel.org/?p=linux%2Fkernel%2Fgit%2Ftorvalds%2Flinux.git;a=commitdiff_plain;h=bfc141e3a515008d85e57af39c9faa4d2bbc65e0;hp=ddf536d0d7e1f0b63a681c970888730a4437414d

ARM: OMAP4: hwmod: Don't wait for the idle status if modulemode is not supported

If the module does not have any modulemode, the _disable_module function
will do nothing. There is then no point waiting for a idle status change.

It will remove the following warnings.

[    0.331848] omap_hwmod: dmm: _wait_target_disable failed
[    0.339935] omap_hwmod: emif_fw: _wait_target_disable failed
[    0.348358] omap_hwmod: l3_main_1: _wait_target_disable failed
[    0.356964] omap_hwmod: l3_main_2: _wait_target_disable failed
[    0.365600] omap_hwmod: l4_abe: _wait_target_disable failed
[    0.373931] omap_hwmod: l4_cfg: _wait_target_disable failed
[    0.382263] omap_hwmod: l4_per: _wait_target_disable failed
[    0.391113] omap_hwmod: l4_wkup: _wait_target_disable failed
[    0.399536] omap_hwmod: dma_system: _wait_target_disable failed
[    0.408325] omap_hwmod: dss_core: _wait_target_disable failed
[    0.416839] omap_hwmod: dss_dispc: _wait_target_disable failed
[    0.425445] omap_hwmod: dss_dsi1: _wait_target_disable failed
[    0.433990] omap_hwmod: dss_dsi2: _wait_target_disable failed
[    0.442504] omap_hwmod: dss_hdmi: _wait_target_disable failed
[    0.451019] omap_hwmod: dss_rfbi: _wait_target_disable failed
[    0.459564] omap_hwmod: dss_venc: _wait_target_disable failed
[    0.489471] omap_hwmod: mailbox: _wait_target_disable failed
[    0.505920] omap_hwmod: spinlock: _wait_target_disable failed

Note: For such module, the state is managed automatically by HW according
to clock domain transition. It is then not possible to wait for idle even
later in the _idle function since the status will change at clock domain
boundary.

Signed-off-by: Benoit Cousson <b-cousson@ti.com>
Cc: Paul Walmsley <paul@pwsan.com>
Cc: Rajendra Nayak <rnayak@ti.com>
[paul@pwsan.com: renamed fns to indicate that they are OMAP4-only; moved
 _wait_target_disable() into _disable_module(), removing duplicate code]
Signed-off-by: Paul Walmsley <paul@pwsan.com>
Signed-off-by: Tony Lindgren <tony@atomide.com>
---

--- a/arch/arm/mach-omap2/omap_hwmod.c
+++ b/arch/arm/mach-omap2/omap_hwmod.c
@@ -706,27 +706,65 @@ static void _enable_module(struct omap_h
 }
 
 /**
- * _disable_module - enable CLKCTRL modulemode on OMAP4
+ * _omap4_wait_target_disable - wait for a module to be disabled on OMAP4
+ * @oh: struct omap_hwmod *
+ *
+ * Wait for a module @oh to enter slave idle.  Returns 0 if the module
+ * does not have an IDLEST bit or if the module successfully enters
+ * slave idle; otherwise, pass along the return value of the
+ * appropriate *_cm*_wait_module_idle() function.
+ */
+static int _omap4_wait_target_disable(struct omap_hwmod *oh)
+{
+	if (!cpu_is_omap44xx())
+		return 0;
+
+	if (!oh)
+		return -EINVAL;
+
+	if (oh->_int_flags & _HWMOD_NO_MPU_PORT)
+		return 0;
+
+	if (oh->flags & HWMOD_NO_IDLEST)
+		return 0;
+
+	return omap4_cminst_wait_module_idle(oh->clkdm->prcm_partition,
+					     oh->clkdm->cm_inst,
+					     oh->clkdm->clkdm_offs,
+					     oh->prcm.omap4.clkctrl_offs);
+}
+
+/**
+ * _omap4_disable_module - enable CLKCTRL modulemode on OMAP4
  * @oh: struct omap_hwmod *
  *
  * Disable the PRCM module mode related to the hwmod @oh.
- * No return value.
+ * Return EINVAL if the modulemode is not supported and 0 in case of success.
  */
-static void _disable_module(struct omap_hwmod *oh)
+static int _omap4_disable_module(struct omap_hwmod *oh)
 {
+	int v;
+
 	/* The module mode does not exist prior OMAP4 */
-	if (cpu_is_omap24xx() || cpu_is_omap34xx())
-		return;
+	if (!cpu_is_omap44xx())
+		return -EINVAL;
 
 	if (!oh->clkdm || !oh->prcm.omap4.modulemode)
-		return;
+		return -EINVAL;
 
-	pr_debug("omap_hwmod: %s: _disable_module\n", oh->name);
+	pr_debug("omap_hwmod: %s: %s\n", oh->name, __func__);
 
 	omap4_cminst_module_disable(oh->clkdm->prcm_partition,
 				    oh->clkdm->cm_inst,
 				    oh->clkdm->clkdm_offs,
 				    oh->prcm.omap4.clkctrl_offs);
+
+	v = _omap4_wait_target_disable(oh);
+	if (v)
+		pr_warn("omap_hwmod: %s: _wait_target_disable failed\n",
+			oh->name);
+
+	return 0;
 }
 
 /**
@@ -1153,36 +1191,6 @@ static int _wait_target_ready(struct oma
 }
 
 /**
- * _wait_target_disable - wait for a module to be disabled
- * @oh: struct omap_hwmod *
- *
- * Wait for a module @oh to enter slave idle.  Returns 0 if the module
- * does not have an IDLEST bit or if the module successfully enters
- * slave idle; otherwise, pass along the return value of the
- * appropriate *_cm*_wait_module_idle() function.
- */
-static int _wait_target_disable(struct omap_hwmod *oh)
-{
-	/* TODO: For now just handle OMAP4+ */
-	if (cpu_is_omap24xx() || cpu_is_omap34xx())
-		return 0;
-
-	if (!oh)
-		return -EINVAL;
-
-	if (oh->_int_flags & _HWMOD_NO_MPU_PORT)
-		return 0;
-
-	if (oh->flags & HWMOD_NO_IDLEST)
-		return 0;
-
-	return omap4_cminst_wait_module_idle(oh->clkdm->prcm_partition,
-					     oh->clkdm->cm_inst,
-					     oh->clkdm->clkdm_offs,
-					     oh->prcm.omap4.clkctrl_offs);
-}
-
-/**
  * _lookup_hardreset - fill register bit info for this hwmod/reset line
  * @oh: struct omap_hwmod *
  * @name: name of the reset line in the context of this hwmod
@@ -1524,8 +1532,6 @@ static int _enable(struct omap_hwmod *oh
  */
 static int _idle(struct omap_hwmod *oh)
 {
-	int ret;
-
 	pr_debug("omap_hwmod: %s: idling\n", oh->name);
 
 	if (oh->_state != _HWMOD_STATE_ENABLED) {
@@ -1537,11 +1543,9 @@ static int _idle(struct omap_hwmod *oh)
 	if (oh->class->sysc)
 		_idle_sysc(oh);
 	_del_initiator_dep(oh, mpu_oh);
-	_disable_module(oh);
-	ret = _wait_target_disable(oh);
-	if (ret)
-		pr_warn("omap_hwmod: %s: _wait_target_disable failed\n",
-			oh->name);
+
+	_omap4_disable_module(oh);
+
 	/*
 	 * The module must be in idle mode before disabling any parents
 	 * clocks. Otherwise, the parent clock might be disabled before
@@ -1642,11 +1646,7 @@ static int _shutdown(struct omap_hwmod *
 	if (oh->_state == _HWMOD_STATE_ENABLED) {
 		_del_initiator_dep(oh, mpu_oh);
 		/* XXX what about the other system initiators here? dma, dsp */
-		_disable_module(oh);
-		ret = _wait_target_disable(oh);
-		if (ret)
-			pr_warn("omap_hwmod: %s: _wait_target_disable failed\n",
-				oh->name);
+		_omap4_disable_module(oh);
 		_disable_clocks(oh);
 		if (oh->clkdm)
 			clkdm_hwmod_disable(oh->clkdm, oh);
