From 7b90e7040b9783b91a4e2baf72ac32d3a00f9f2d Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Sat, 21 Jan 2012 11:18:25 +0100
Subject: [PATCH 31/34] ssb: fix cardbus in hostmode


Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 drivers/ssb/driver_pcicore.c |    2 +-
 1 files changed, 1 insertions(+), 1 deletions(-)

--- a/drivers/ssb/driver_pcicore.c
+++ b/drivers/ssb/driver_pcicore.c
@@ -75,7 +75,7 @@ static u32 get_cfgspace_addr(struct ssb_
 	u32 tmp;
 
 	/* We do only have one cardbus device behind the bridge. */
-	if (pc->cardbusmode && (dev >= 1))
+	if (pc->cardbusmode && (dev > 1))
 		goto out;
 
 	if (bus == 0) {
