From 00624e5d91c0e76f38730633eff51fc7630dd27b Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Mon, 20 Jun 2011 21:26:05 +0200
Subject: [PATCH 08/27] MIPS: ath79: Add AR933X specific glue for ath79_device_reset_{set,clear}

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
Cc: linux-mips@linux-mips.org
Cc: Kathy Giori <kgiori@qca.qualcomm.com>
Cc: "Luis R.  Rodriguez" <rodrigue@qca.qualcomm.com>
Patchwork: https://patchwork.linux-mips.org/patch/2523/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ath79/common.c                       |    4 ++++
 arch/mips/include/asm/mach-ath79/ar71xx_regs.h |    1 +
 2 files changed, 5 insertions(+), 0 deletions(-)

--- a/arch/mips/ath79/common.c
+++ b/arch/mips/ath79/common.c
@@ -64,6 +64,8 @@ void ath79_device_reset_set(u32 mask)
 		reg = AR724X_RESET_REG_RESET_MODULE;
 	else if (soc_is_ar913x())
 		reg = AR913X_RESET_REG_RESET_MODULE;
+	else if (soc_is_ar933x())
+		reg = AR933X_RESET_REG_RESET_MODULE;
 	else
 		BUG();
 
@@ -86,6 +88,8 @@ void ath79_device_reset_clear(u32 mask)
 		reg = AR724X_RESET_REG_RESET_MODULE;
 	else if (soc_is_ar913x())
 		reg = AR913X_RESET_REG_RESET_MODULE;
+	else if (soc_is_ar933x())
+		reg = AR933X_RESET_REG_RESET_MODULE;
 	else
 		BUG();
 
--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -173,6 +173,7 @@
 
 #define AR724X_RESET_REG_RESET_MODULE		0x1c
 
+#define AR933X_RESET_REG_RESET_MODULE		0x1c
 #define AR933X_RESET_REG_BOOTSTRAP		0xac
 
 #define MISC_INT_ETHSW			BIT(12)
