From 744ffdd4e90cd6671f46eadf9d7cf55b07618d73 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Fri, 18 Nov 2011 21:37:17 +0100
Subject: [PATCH 09/35] MIPS: ath79: remove superfluous alignment checks from pci-ar724x.c

The alignment of the 'where' parameters are checked
in the core PCI code already.

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>

v2: - no changes
---
 arch/mips/pci/pci-ar724x.c |    6 ------
 1 files changed, 0 insertions(+), 6 deletions(-)

--- a/arch/mips/pci/pci-ar724x.c
+++ b/arch/mips/pci/pci-ar724x.c
@@ -28,9 +28,6 @@ static int ar724x_pci_read(struct pci_bu
 	if (devfn)
 		return PCIBIOS_DEVICE_NOT_FOUND;
 
-	if (where & (size - 1))
-		return PCIBIOS_BAD_REGISTER_NUMBER;
-
 	base = ar724x_pci_devcfg_base;
 
 	spin_lock_irqsave(&ar724x_pci_lock, flags);
@@ -73,9 +70,6 @@ static int ar724x_pci_write(struct pci_b
 	if (devfn)
 		return PCIBIOS_DEVICE_NOT_FOUND;
 
-	if (where & (size - 1))
-		return PCIBIOS_BAD_REGISTER_NUMBER;
-
 	base = ar724x_pci_devcfg_base;
 
 	spin_lock_irqsave(&ar724x_pci_lock, flags);
