From d3fb63a710e1f04fed2c2703c6dce3531490c451 Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Mon, 6 Jun 2011 00:07:37 +0200
Subject: [PATCH 10/26] bcm47xx: add support for bcma bus

This patch add support for the bcma bus. Broadcom uses only Mips 74K
CPUs on the new SoC and on the old ons using ssb bus there are no Mips
74K CPUs.

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 arch/mips/bcm47xx/Kconfig                    |   13 ++++++
 arch/mips/bcm47xx/gpio.c                     |   22 +++++++++++
 arch/mips/bcm47xx/nvram.c                    |   10 +++++
 arch/mips/bcm47xx/serial.c                   |   29 ++++++++++++++
 arch/mips/bcm47xx/setup.c                    |   53 +++++++++++++++++++++++++-
 arch/mips/bcm47xx/time.c                     |    5 ++
 arch/mips/include/asm/mach-bcm47xx/bcm47xx.h |    8 ++++
 arch/mips/include/asm/mach-bcm47xx/gpio.h    |   41 ++++++++++++++++++++
 drivers/watchdog/bcm47xx_wdt.c               |   11 +++++
 9 files changed, 190 insertions(+), 2 deletions(-)

--- a/arch/mips/bcm47xx/Kconfig
+++ b/arch/mips/bcm47xx/Kconfig
@@ -15,4 +15,17 @@ config BCM47XX_SSB
 
 	 This will generate an image with support for SSB and MIPS32 R1 instruction set.
 
+config BCM47XX_BCMA
+	bool "BCMA Support for Broadcom BCM47XX"
+	select SYS_HAS_CPU_MIPS32_R2
+	select BCMA
+	select BCMA_HOST_SOC
+	select BCMA_DRIVER_MIPS
+	select BCMA_DRIVER_PCI_HOSTMODE if PCI
+	default y
+	help
+	 Add support for new Broadcom BCM47xx boards with Broadcom specific Advanced Microcontroller Bus.
+
+	 This will generate an image with support for BCMA and MIPS32 R2 instruction set.
+
 endif
--- a/arch/mips/bcm47xx/gpio.c
+++ b/arch/mips/bcm47xx/gpio.c
@@ -36,6 +36,16 @@ int gpio_request(unsigned gpio, const ch
 
 		return 0;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		if (gpio >= BCM47XX_CHIPCO_GPIO_LINES)
+			return -EINVAL;
+
+		if (test_and_set_bit(gpio, gpio_in_use))
+			return -EBUSY;
+
+		return 0;
+#endif
 	}
 	return -EINVAL;
 }
@@ -57,6 +67,14 @@ void gpio_free(unsigned gpio)
 		clear_bit(gpio, gpio_in_use);
 		return;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		if (gpio >= BCM47XX_CHIPCO_GPIO_LINES)
+			return;
+
+		clear_bit(gpio, gpio_in_use);
+		return;
+#endif
 	}
 }
 EXPORT_SYMBOL(gpio_free);
@@ -73,6 +91,10 @@ int gpio_to_irq(unsigned gpio)
 		else
 			return -EINVAL;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		return bcma_core_mips_irq(bcm47xx_bus.bcma.bus.drv_cc.core) + 2;
+#endif
 	}
 	return -EINVAL;
 }
--- a/arch/mips/bcm47xx/nvram.c
+++ b/arch/mips/bcm47xx/nvram.c
@@ -29,6 +29,9 @@ static void early_nvram_init(void)
 #ifdef CONFIG_BCM47XX_SSB
 	struct ssb_mipscore *mcore_ssb;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	struct bcma_drv_cc *bcma_cc;
+#endif
 	struct nvram_header *header;
 	int i;
 	u32 base = 0;
@@ -44,6 +47,13 @@ static void early_nvram_init(void)
 		lim = mcore_ssb->flash_window_size;
 		break;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_cc = &bcm47xx_bus.bcma.bus.drv_cc;
+		base = bcma_cc->pflash.window;
+		lim = bcma_cc->pflash.window_size;
+		break;
+#endif
 	}
 
 	off = FLASH_MIN;
--- a/arch/mips/bcm47xx/serial.c
+++ b/arch/mips/bcm47xx/serial.c
@@ -47,6 +47,31 @@ static int __init uart8250_init_ssb(void
 }
 #endif
 
+#ifdef CONFIG_BCM47XX_BCMA
+static int __init uart8250_init_bcma(void)
+{
+	int i;
+	struct bcma_drv_cc *cc = &(bcm47xx_bus.bcma.bus.drv_cc);
+
+	memset(&uart8250_data, 0,  sizeof(uart8250_data));
+
+	for (i = 0; i < cc->nr_serial_ports; i++) {
+		struct plat_serial8250_port *p = &(uart8250_data[i]);
+		struct bcma_serial_port *bcma_port;
+		bcma_port = &(cc->serial_ports[i]);
+
+		p->mapbase = (unsigned int) bcma_port->regs;
+		p->membase = (void *) bcma_port->regs;
+		p->irq = bcma_port->irq + 2;
+		p->uartclk = bcma_port->baud_base;
+		p->regshift = bcma_port->reg_shift;
+		p->iotype = UPIO_MEM;
+		p->flags = UPF_BOOT_AUTOCONF | UPF_SHARE_IRQ;
+	}
+	return platform_device_register(&uart8250_device);
+}
+#endif
+
 static int __init uart8250_init(void)
 {
 	switch (bcm47xx_bus_type) {
@@ -54,6 +79,10 @@ static int __init uart8250_init(void)
 	case BCM47XX_BUS_TYPE_SSB:
 		return uart8250_init_ssb();
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		return uart8250_init_bcma();
+#endif
 	}
 	return -EINVAL;
 }
--- a/arch/mips/bcm47xx/setup.c
+++ b/arch/mips/bcm47xx/setup.c
@@ -29,6 +29,7 @@
 #include <linux/types.h>
 #include <linux/ssb/ssb.h>
 #include <linux/ssb/ssb_embedded.h>
+#include <linux/bcma/bcma_soc.h>
 #include <asm/bootinfo.h>
 #include <asm/reboot.h>
 #include <asm/time.h>
@@ -52,6 +53,11 @@ static void bcm47xx_machine_restart(char
 		ssb_watchdog_timer_set(&bcm47xx_bus.ssb, 1);
 		break;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_chipco_watchdog_timer_set(&bcm47xx_bus.bcma.bus.drv_cc, 1);
+		break;
+#endif
 	}
 	while (1)
 		cpu_relax();
@@ -67,6 +73,11 @@ static void bcm47xx_machine_halt(void)
 		ssb_watchdog_timer_set(&bcm47xx_bus.ssb, 0);
 		break;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_chipco_watchdog_timer_set(&bcm47xx_bus.bcma.bus.drv_cc, 0);
+		break;
+#endif
 	}
 	while (1)
 		cpu_relax();
@@ -295,16 +306,54 @@ static void __init bcm47xx_register_ssb(
 }
 #endif
 
+#ifdef CONFIG_BCM47XX_BCMA
+static void __init bcm47xx_register_bcma(void)
+{
+	int err;
+
+	err = bcma_host_soc_register(&bcm47xx_bus.bcma);
+	if (err)
+		panic("Failed to initialize BCMA bus (err %d)\n", err);
+}
+#endif
+
 void __init plat_mem_setup(void)
 {
 	struct cpuinfo_mips *c = &current_cpu_data;
 
+	if (c->cputype == CPU_74K) {
+		printk(KERN_INFO "bcm47xx: using bcma bus\n");
+#ifdef CONFIG_BCM47XX_BCMA
+		bcm47xx_bus_type = BCM47XX_BUS_TYPE_BCMA;
+		bcm47xx_register_bcma();
+#endif
+	} else {
+		printk(KERN_INFO "bcm47xx: using ssb bus\n");
 #ifdef CONFIG_BCM47XX_SSB
-	bcm47xx_bus_type = BCM47XX_BUS_TYPE_SSB;
-	bcm47xx_register_ssb();
+		bcm47xx_bus_type = BCM47XX_BUS_TYPE_SSB;
+		bcm47xx_register_ssb();
 #endif
+	}
 
 	_machine_restart = bcm47xx_machine_restart;
 	_machine_halt = bcm47xx_machine_halt;
 	pm_power_off = bcm47xx_machine_halt;
 }
+
+static int __init bcm47xx_register_bus_complete(void)
+{
+	switch (bcm47xx_bus_type) {
+#ifdef CONFIG_BCM47XX_SSB
+	case BCM47XX_BUS_TYPE_SSB:
+		/* Nothing to do */
+		break;
+#endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_bus_register(&bcm47xx_bus.bcma.bus);
+		break;
+#endif
+	}
+	return 0;
+}
+device_initcall(bcm47xx_register_bus_complete);
--- a/arch/mips/bcm47xx/time.c
+++ b/arch/mips/bcm47xx/time.c
@@ -45,6 +45,11 @@ void __init plat_time_init(void)
 		hz = ssb_cpu_clock(&bcm47xx_bus.ssb.mipscore) / 2;
 		break;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		hz = bcma_cpu_clock(&bcm47xx_bus.bcma.bus.drv_mips) / 2;
+		break;
+#endif
 	}
 
 	if (!hz)
--- a/arch/mips/include/asm/mach-bcm47xx/bcm47xx.h
+++ b/arch/mips/include/asm/mach-bcm47xx/bcm47xx.h
@@ -20,17 +20,25 @@
 #define __ASM_BCM47XX_H
 
 #include <linux/ssb/ssb.h>
+#include <linux/bcma/bcma.h>
+#include <linux/bcma/bcma_soc.h>
 
 enum bcm47xx_bus_type {
 #ifdef CONFIG_BCM47XX_SSB
 	BCM47XX_BUS_TYPE_SSB,
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	BCM47XX_BUS_TYPE_BCMA,
+#endif
 };
 
 union bcm47xx_bus {
 #ifdef CONFIG_BCM47XX_SSB
 	struct ssb_bus ssb;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	struct bcma_soc bcma;
+#endif
 };
 
 extern union bcm47xx_bus bcm47xx_bus;
--- a/arch/mips/include/asm/mach-bcm47xx/gpio.h
+++ b/arch/mips/include/asm/mach-bcm47xx/gpio.h
@@ -10,6 +10,7 @@
 #define __BCM47XX_GPIO_H
 
 #include <linux/ssb/ssb_embedded.h>
+#include <linux/bcma/bcma.h>
 #include <asm/mach-bcm47xx/bcm47xx.h>
 
 #define BCM47XX_EXTIF_GPIO_LINES	5
@@ -26,6 +27,11 @@ static inline int gpio_get_value(unsigne
 	case BCM47XX_BUS_TYPE_SSB:
 		return ssb_gpio_in(&bcm47xx_bus.ssb, 1 << gpio);
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		return bcma_chipco_gpio_in(&bcm47xx_bus.bcma.bus.drv_cc,
+					   1 << gpio);
+#endif
 	}
 	return -EINVAL;
 }
@@ -37,6 +43,13 @@ static inline void gpio_set_value(unsign
 	case BCM47XX_BUS_TYPE_SSB:
 		ssb_gpio_out(&bcm47xx_bus.ssb, 1 << gpio,
 			     value ? 1 << gpio : 0);
+		return;
+#endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_chipco_gpio_out(&bcm47xx_bus.bcma.bus.drv_cc, 1 << gpio,
+				     value ? 1 << gpio : 0);
+		return;
 #endif
 	}
 }
@@ -49,6 +62,12 @@ static inline int gpio_direction_input(u
 		ssb_gpio_outen(&bcm47xx_bus.ssb, 1 << gpio, 0);
 		return 0;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_chipco_gpio_outen(&bcm47xx_bus.bcma.bus.drv_cc, 1 << gpio,
+				       0);
+		return 0;
+#endif
 	}
 	return -EINVAL;
 }
@@ -65,6 +84,16 @@ static inline int gpio_direction_output(
 		ssb_gpio_outen(&bcm47xx_bus.ssb, 1 << gpio, 1 << gpio);
 		return 0;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		/* first set the gpio out value */
+		bcma_chipco_gpio_out(&bcm47xx_bus.bcma.bus.drv_cc, 1 << gpio,
+				     value ? 1 << gpio : 0);
+		/* then set the gpio mode */
+		bcma_chipco_gpio_outen(&bcm47xx_bus.bcma.bus.drv_cc, 1 << gpio,
+				       1 << gpio);
+		return 0;
+#endif
 	}
 	return -EINVAL;
 }
@@ -78,6 +107,12 @@ static inline int gpio_intmask(unsigned
 				 value ? 1 << gpio : 0);
 		return 0;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_chipco_gpio_intmask(&bcm47xx_bus.bcma.bus.drv_cc,
+					 1 << gpio, value ? 1 << gpio : 0);
+		return 0;
+#endif
 	}
 	return -EINVAL;
 }
@@ -91,6 +126,12 @@ static inline int gpio_polarity(unsigned
 				  value ? 1 << gpio : 0);
 		return 0;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_chipco_gpio_polarity(&bcm47xx_bus.bcma.bus.drv_cc,
+					  1 << gpio, value ? 1 << gpio : 0);
+		return 0;
+#endif
 	}
 	return -EINVAL;
 }
--- a/drivers/watchdog/bcm47xx_wdt.c
+++ b/drivers/watchdog/bcm47xx_wdt.c
@@ -60,6 +60,12 @@ static inline void bcm47xx_wdt_hw_start(
 		ssb_watchdog_timer_set(&bcm47xx_bus.ssb, 0xfffffff);
 		break;
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_chipco_watchdog_timer_set(&bcm47xx_bus.bcma.bus.drv_cc,
+					       0xfffffff);
+		break;
+#endif
 	}
 }
 
@@ -70,6 +76,11 @@ static inline int bcm47xx_wdt_hw_stop(vo
 	case BCM47XX_BUS_TYPE_SSB:
 		return ssb_watchdog_timer_set(&bcm47xx_bus.ssb, 0);
 #endif
+#ifdef CONFIG_BCM47XX_BCMA
+	case BCM47XX_BUS_TYPE_BCMA:
+		bcma_chipco_watchdog_timer_set(&bcm47xx_bus.bcma.bus.drv_cc, 0);
+		return 0;
+#endif
 	}
 	return -EINVAL;
 }
