From f2963f6a811da75e2531fd1312aa124cd73f15d5 Mon Sep 17 00:00:00 2001
From: Gabor Juhos <juhosg@openwrt.org>
Date: Mon, 20 Jun 2011 21:26:06 +0200
Subject: [PATCH 09/27] MIPS: ath79: Add AR933X specific IRQ initialization

Signed-off-by: Gabor Juhos <juhosg@openwrt.org>
Cc: linux-mips@linux-mips.org
Cc: Kathy Giori <kgiori@qca.qualcomm.com>
Cc: "Luis R.  Rodriguez" <rodrigue@qca.qualcomm.com>
Patchwork: https://patchwork.linux-mips.org/patch/2530/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ath79/irq.c                          |    5 ++++-
 arch/mips/include/asm/mach-ath79/ar71xx_regs.h |    5 +++++
 2 files changed, 9 insertions(+), 1 deletions(-)

--- a/arch/mips/ath79/irq.c
+++ b/arch/mips/ath79/irq.c
@@ -129,7 +129,7 @@ static void __init ath79_misc_irq_init(v
 
 	if (soc_is_ar71xx() || soc_is_ar913x())
 		ath79_misc_irq_chip.irq_mask_ack = ar71xx_misc_irq_mask;
-	else if (soc_is_ar724x())
+	else if (soc_is_ar724x() || soc_is_ar933x())
 		ath79_misc_irq_chip.irq_ack = ar724x_misc_irq_ack;
 	else
 		BUG();
@@ -186,6 +186,9 @@ void __init arch_init_irq(void)
 	} else if (soc_is_ar913x()) {
 		ath79_ip2_flush_reg = AR913X_DDR_REG_FLUSH_WMAC;
 		ath79_ip3_flush_reg = AR913X_DDR_REG_FLUSH_USB;
+	} else if (soc_is_ar933x()) {
+		ath79_ip2_flush_reg = AR933X_DDR_REG_FLUSH_WMAC;
+		ath79_ip3_flush_reg = AR933X_DDR_REG_FLUSH_USB;
 	} else
 		BUG();
 
--- a/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
+++ b/arch/mips/include/asm/mach-ath79/ar71xx_regs.h
@@ -82,6 +82,11 @@
 #define AR913X_DDR_REG_FLUSH_USB	0x84
 #define AR913X_DDR_REG_FLUSH_WMAC	0x88
 
+#define AR933X_DDR_REG_FLUSH_GE0	0x7c
+#define AR933X_DDR_REG_FLUSH_GE1	0x80
+#define AR933X_DDR_REG_FLUSH_USB	0x84
+#define AR933X_DDR_REG_FLUSH_WMAC	0x88
+
 /*
  * PLL block
  */
