This patch adds a new GPIO driver for the RDC321x SoC GPIO controller.

Signed-off-by: Florian Fainelli <florian@openwrt.org>
---
Changes from v2:
- initialize spinlock earlier
- do not declare and assign gpch variables on the same line
- use the pci_dev pointer passed as platform data
- replaced rdc321x_pci_{read,write}

--- a/drivers/gpio/Kconfig
+++ b/drivers/gpio/Kconfig
@@ -196,6 +196,14 @@ config GPIO_LANGWELL
 	help
 	  Say Y here to support Intel Moorestown platform GPIO.
 
+config GPIO_RDC321X
+	tristate "RDC R-321x GPIO support"
+	depends on PCI && GPIOLIB
+	select MFD_RDC321X
+	help
+	  Support for the RDC R321x SoC GPIOs over southbridge
+	  PCI configuration space.
+
 comment "SPI GPIO expanders:"
 
 config GPIO_MAX7301
--- a/drivers/gpio/Makefile
+++ b/drivers/gpio/Makefile
@@ -19,3 +19,4 @@ obj-$(CONFIG_GPIO_XILINX)	+= xilinx_gpio
 obj-$(CONFIG_GPIO_BT8XX)	+= bt8xxgpio.o
 obj-$(CONFIG_GPIO_VR41XX)	+= vr41xx_giu.o
 obj-$(CONFIG_GPIO_WM831X)	+= wm831x-gpio.o
+obj-$(CONFIG_GPIO_RDC321X)	+= rdc321x-gpio.o
--- /dev/null
+++ b/drivers/gpio/rdc321x-gpio.c
@@ -0,0 +1,245 @@
+/*
+ * RDC321x GPIO driver
+ *
+ * Copyright (C) 2008, Volker Weiss <dev@tintuc.de>
+ * Copyright (C) 2007-2010 Florian Fainelli <florian@openwrt.org>
+ *
+ * This program is free software; you can redistribute it and/or modify
+ * it under the terms of the GNU General Public License as published by
+ * the Free Software Foundation; either version 2 of the License, or
+ * (at your option) any later version.
+ *
+ * This program is distributed in the hope that it will be useful,
+ * but WITHOUT ANY WARRANTY; without even the implied warranty of
+ * MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ * GNU General Public License for more details.
+ *
+ * You should have received a copy of the GNU General Public License
+ * along with this program; if not, write to the Free Software
+ * Foundation, Inc., 675 Mass Ave, Cambridge, MA 02139, USA.
+ *
+ */
+#include <linux/module.h>
+#include <linux/kernel.h>
+#include <linux/init.h>
+#include <linux/spinlock.h>
+#include <linux/platform_device.h>
+#include <linux/pci.h>
+#include <linux/gpio.h>
+#include <linux/mfd/rdc321x.h>
+
+struct rdc321x_gpio {
+	spinlock_t		lock;
+	struct pci_dev		*sb_pdev;
+	u32			data_reg[2];
+	int			reg1_ctrl_base;
+	int			reg1_data_base;
+	int			reg2_ctrl_base;
+	int			reg2_data_base;
+	struct gpio_chip	chip;
+};
+
+/* read GPIO pin */
+static int rdc_gpio_get_value(struct gpio_chip *chip, unsigned gpio)
+{
+	struct rdc321x_gpio *gpch;
+	u32 value = 0;
+	int reg;
+
+	gpch = container_of(chip, struct rdc321x_gpio, chip);
+	reg = gpio < 32 ? gpch->reg1_data_base : gpch->reg2_data_base;
+
+	spin_lock(&gpch->lock);
+	pci_write_config_dword(gpch->sb_pdev, reg,
+					gpch->data_reg[gpio < 32 ? 0 : 1]);
+	pci_read_config_dword(gpch->sb_pdev, reg, &value);
+	spin_unlock(&gpch->lock);
+
+	return (1 << (gpio & 0x1f)) & value ? 1 : 0;
+}
+
+static void rdc_gpio_set_value_impl(struct gpio_chip *chip,
+				unsigned gpio, int value)
+{
+	struct rdc321x_gpio *gpch;
+	int reg = (gpio < 32) ? 0 : 1;
+
+	gpch = container_of(chip, struct rdc321x_gpio, chip);
+
+	if (value)
+		gpch->data_reg[reg] |= 1 << (gpio & 0x1f);
+	else
+		gpch->data_reg[reg] &= ~(1 << (gpio & 0x1f));
+
+	pci_write_config_dword(gpch->sb_pdev,
+			reg ? gpch->reg2_data_base : gpch->reg1_data_base,
+			gpch->data_reg[reg]);
+}
+
+/* set GPIO pin to value */
+static void rdc_gpio_set_value(struct gpio_chip *chip,
+				unsigned gpio, int value)
+{
+	struct rdc321x_gpio *gpch;
+
+	gpch = container_of(chip, struct rdc321x_gpio, chip);
+	spin_lock(&gpch->lock);
+	rdc_gpio_set_value_impl(chip, gpio, value);
+	spin_unlock(&gpch->lock);
+}
+
+static int rdc_gpio_config(struct gpio_chip *chip,
+				unsigned gpio, int value)
+{
+	struct rdc321x_gpio *gpch;
+	int err;
+	u32 reg;
+
+	gpch = container_of(chip, struct rdc321x_gpio, chip);
+
+	spin_lock(&gpch->lock);
+	err = pci_read_config_dword(gpch->sb_pdev, gpio < 32 ?
+			gpch->reg1_ctrl_base : gpch->reg2_ctrl_base, &reg);
+	if (err)
+		goto unlock;
+
+	reg |= 1 << (gpio & 0x1f);
+
+	err = pci_write_config_dword(gpch->sb_pdev, gpio < 32 ?
+			gpch->reg1_ctrl_base : gpch->reg2_ctrl_base, reg);
+	if (err)
+		goto unlock;
+
+	rdc_gpio_set_value_impl(chip, gpio, value);
+
+unlock:
+	spin_unlock(&gpch->lock);
+
+	return err;
+}
+
+/* configure GPIO pin as input */
+static int rdc_gpio_direction_input(struct gpio_chip *chip, unsigned gpio)
+{
+	return rdc_gpio_config(chip, gpio, 1);
+}
+
+/*
+ * Cache the initial value of both GPIO data registers
+ */
+static int __devinit rdc321x_gpio_probe(struct platform_device *pdev)
+{
+	int err;
+	struct resource *r;
+	struct rdc321x_gpio *rdc321x_gpio_dev;
+	struct rdc321x_gpio_pdata *pdata;
+
+	pdata = platform_get_drvdata(pdev);
+	if (!pdata) {
+		dev_err(&pdev->dev, "no platform data supplied\n");
+		return -ENODEV;
+	}
+
+	rdc321x_gpio_dev = kzalloc(sizeof(struct rdc321x_gpio), GFP_KERNEL);
+	if (!rdc321x_gpio_dev) {
+		dev_err(&pdev->dev, "failed to allocate private data\n");
+		return -ENOMEM;
+	}
+
+	r = platform_get_resource_byname(pdev, IORESOURCE_IO, "gpio-reg1");
+	if (!r) {
+		dev_err(&pdev->dev, "failed to get gpio-reg1 resource\n");
+		err = -ENODEV;
+		goto out_free;
+	}
+
+	spin_lock_init(&rdc321x_gpio_dev->lock);
+	rdc321x_gpio_dev->sb_pdev = pdata->sb_pdev;
+	rdc321x_gpio_dev->reg1_ctrl_base = r->start;
+	rdc321x_gpio_dev->reg1_data_base = r->start + 0x4;
+
+	r = platform_get_resource_byname(pdev, IORESOURCE_IO, "gpio-reg2");
+	if (!r) {
+		dev_err(&pdev->dev, "failed to get gpio-reg2 resource\n");
+		err = -ENODEV;
+		goto out_free;
+	}
+
+	rdc321x_gpio_dev->reg2_ctrl_base = r->start;
+	rdc321x_gpio_dev->reg2_data_base = r->start + 0x4;
+
+	rdc321x_gpio_dev->chip.label = "rdc321x-gpio";
+	rdc321x_gpio_dev->chip.direction_input = rdc_gpio_direction_input;
+	rdc321x_gpio_dev->chip.direction_output = rdc_gpio_config;
+	rdc321x_gpio_dev->chip.get = rdc_gpio_get_value;
+	rdc321x_gpio_dev->chip.set = rdc_gpio_set_value;
+	rdc321x_gpio_dev->chip.base = 0;
+	rdc321x_gpio_dev->chip.ngpio = pdata->max_gpios;
+
+	platform_set_drvdata(pdev, rdc321x_gpio_dev);
+
+	/* This might not be, what others (BIOS, bootloader, etc.)
+	   wrote to these registers before, but it's a good guess. Still
+	   better than just using 0xffffffff. */
+	err = pci_read_config_dword(rdc321x_gpio_dev->sb_pdev,
+					rdc321x_gpio_dev->reg1_data_base,
+					&rdc321x_gpio_dev->data_reg[0]);
+	if (err)
+		goto out_drvdata;
+
+	err = pci_read_config_dword(rdc321x_gpio_dev->sb_pdev,
+					rdc321x_gpio_dev->reg2_data_base,
+					&rdc321x_gpio_dev->data_reg[1]);
+	if (err)
+		goto out_drvdata;
+
+	dev_info(&pdev->dev, "registering %d GPIOs\n",
+					rdc321x_gpio_dev->chip.ngpio);
+	return gpiochip_add(&rdc321x_gpio_dev->chip);
+
+out_drvdata:
+	platform_set_drvdata(pdev, NULL);
+out_free:
+	kfree(rdc321x_gpio_dev);
+	return err;
+}
+
+static int __devexit rdc321x_gpio_remove(struct platform_device *pdev)
+{
+	int ret;
+	struct rdc321x_gpio *rdc321x_gpio_dev = platform_get_drvdata(pdev);
+
+	ret = gpiochip_remove(&rdc321x_gpio_dev->chip);
+	if (ret)
+		dev_err(&pdev->dev, "failed to unregister chip\n");
+
+	kfree(rdc321x_gpio_dev);
+	platform_set_drvdata(pdev, NULL);
+
+	return ret;
+}
+
+static struct platform_driver rdc321x_gpio_driver = {
+	.driver.name	= "rdc321x-gpio",
+	.driver.owner	= THIS_MODULE,
+	.probe		= rdc321x_gpio_probe,
+	.remove		= __devexit_p(rdc321x_gpio_remove),
+};
+
+static int __init rdc321x_gpio_init(void)
+{
+	return platform_driver_register(&rdc321x_gpio_driver);
+}
+
+static void __exit rdc321x_gpio_exit(void)
+{
+	platform_driver_unregister(&rdc321x_gpio_driver);
+}
+
+module_init(rdc321x_gpio_init);
+module_exit(rdc321x_gpio_exit);
+
+MODULE_AUTHOR("Florian Fainelli <florian@openwrt.org>");
+MODULE_DESCRIPTION("RDC321x GPIO driver");
+MODULE_LICENSE("GPL");
+MODULE_ALIAS("platform:rdc321x-gpio");
