--- pcmcia-cs-3.1.34/etc/config.opts.orig	Tue Jul  9 09:36:23 2002
+++ pcmcia-cs-3.1.34/etc/config.opts	Tue Jul  9 09:37:47 2002
@@ -5,7 +5,7 @@
 
 # System resources available for PCMCIA devices
 
-include port 0x100-0x4ff, port 0x800-0x8ff, port 0xc00-0xcff
+include port 0x100-0x4ff, port 0xc00-0xcff
 include memory 0xc0000-0xfffff
 include memory 0xa0000000-0xa0ffffff, memory 0x60000000-0x60ffffff
 
diff -urN pcmcia-cs-3.2.3.orig/etc/shared pcmcia-cs-3.2.3/etc/shared
--- pcmcia-cs-3.2.3.orig/etc/shared	2002-08-18 21:21:11.000000000 -0600
+++ pcmcia-cs-3.2.3/etc/shared	2003-02-14 05:05:07.000000000 -0700
@@ -2,6 +2,8 @@
 # shared 1.31 2002/08/19 03:21:11 (David Hinds)
 #
 
+umask 022
+
 usage ()
 {
     echo "usage: $0 [action] [device name]"
--- /dev/null	2003-01-21 22:14:35.000000000 -0700
+++ pcmcia-cs-3.2.4/etc/pcmcia	2003-06-09 12:04:02.000000000 -0600
@@ -0,0 +1,6 @@
+# Defaults for pcmcia (sourced by /etc/init.d/S30pcmcia)
+PCMCIA=yes
+PCIC=yenta_socket
+PCIC_OPTS=
+CORE_OPTS=
+CARDMGR_OPTS=
--- pcmcia-cs-3.2.4/etc/rc.pcmcia.orig	2002-08-08 00:43:43.000000000 -0600
+++ pcmcia-cs-3.2.4/etc/rc.pcmcia	2003-06-09 15:17:28.000000000 -0600
@@ -4,6 +4,8 @@
 #
 # This is designed to work in BSD as well as SysV init setups.  See
 # the HOWTO for customization instructions.
+# Modified to comply with Debian's standards by Brian Mays
+# <brian@debian.org>.
 
 # Tags for Red Hat init configuration tools
 #
@@ -26,9 +28,9 @@
 done
 
 # Source PCMCIA configuration, if available
-if [ -f /etc/pcmcia.conf ] ; then
+if [ -f /etc/default/pcmcia ] ; then
     # Debian startup option file
-    . /etc/pcmcia.conf
+    . /etc/default/pcmcia
 elif [ -f /etc/sysconfig/pcmcia ] ; then
     # Red Hat startup option file
     . /etc/sysconfig/pcmcia
@@ -50,9 +52,22 @@
 done
 if [ "$PCMCIA" -a "$PCMCIA" != "yes" ] ; then exit 0 ; fi
 
+# Debian modification: Fix PCIC for stand-alone modules.
+# yenta_socket -> i82365 on these systems.
+# Existence of a standalone module implies that it is preferred.
+if [ -d /lib/modules/preferred ] ; then
+    PC=/lib/modules/preferred/pcmcia
+else
+    PC=/lib/modules/`uname -r`/pcmcia
+fi
+if [ "$PCIC" = yenta_socket -a -e $PC/i82365.o \
+    -a ! -L $PC/i82365.o ]; then
+    PCIC=i82365
+fi
+
 usage()
 {
-    echo "Usage: $0 {start|stop|status|restart|reload}"
+    echo "Usage: $0 {start|stop|status|restart|reload|force-reload}"
 }
 
 cleanup()
@@ -84,7 +99,7 @@
 	    SC=/var/lib/pcmcia/scheme
 	    RUN=/var/lib/pcmcia
 	else
-	    SC=/var/run/pcmcia-scheme
+	    SC=/var/lib/misc/pcmcia-scheme
 	    RUN=/var/run
 	fi
 	if [ -L $SC -o ! -O $SC ] ; then rm -f $SC ; fi
@@ -154,7 +172,7 @@
 	;;
 
     status)
-	pid=`/sbin/pidof cardmgr`
+	pid=`/bin/pidof cardmgr`
 	if [ "$pid" != "" ] ; then
 	    echo "cardmgr (pid $pid) is running..."
 	    EXITCODE=0
@@ -164,12 +182,18 @@
 	fi
 	;;
 
-    restart|reload)
+    restart)
 	$0 stop
 	$0 start
 	EXITCODE=$?
 	;;
 
+    reload|force-reload)
+	echo "Reloading $DESC configuration files."
+	kill -1 `cat /var/run/cardmgr.pid` 2>/dev/null
+	EXITCODE=0
+	;;
+
     *)
 	usage
 	;;
@@ -179,4 +203,4 @@
 done
 
 # Only exit if we're in our own subshell
-case $0 in *rc.pcmcia) exit $EXITCODE ;; esac
+case $0 in *pcmcia) exit $EXITCODE ;; esac
